Release 3.2.0

♣ The deadline of tag collector was postponed.

(May 23th).

♣ LArHECTBCnv moved to LArCnv.

♣ LArDigit was updated.

Don’t use Identifier but LArSignalChannelID (one private member (int))

For TestBeam

♣ We use LArHECTBEvent (same class as before).

Move to LArTBEvent for ROOT I/O service after TestBeam

♣ LArHECTBCnv will be updated to simplify for modification. • Code • Class Diagram • Documentation

/afs/cern.ch/user/n/nkanaya/myCVSROOT

→ The first version will be ready in May.

Structure of converter

♣ ./hectb

→ Handle EPIO data ♣ ./src and ./LArHECTBCnv → Convert EPIO data to TDS Six classes for converter

Strucuture of converter

How to update

Basically, three files for one object (bank) • Tobj.h • Alg obj.h • Alg obj.cxx (1) Add new data

How to update

(2) Add new unpacking method